; Silabs USBXpress Driver
; Copyright (c) 2013, Silicon Laboratories

[Version]
Signature = "$Windows NT$"
Class=USB
ClassGUID={36fc9e60-c465-11cf-8056-444553540000}
Provider = %ProviderName%
DriverVer=04/08/2013,4.0.0.0
CatalogFile=siusbxp.cat

; ========== Manufacturer/Models sections ===========

[Manufacturer]
%ProviderName% = USBXpress_WinUSB,NTx86,NTamd64,NTia64

[USBXpress_WinUSB.NTx86]
%USB\VID_10C4&PID_EA61.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61
%USB\VID_10C4&PID_EA61&MI_00.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_00
%USB\VID_10C4&PID_EA61&MI_01.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_01
%USB\VID_10C4&PID_EA61&MI_02.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_02
%USB\VID_10C4&PID_EA61&MI_03.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_03

[USBXpress_WinUSB.NTamd64]
%USB\VID_10C4&PID_EA61.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61
%USB\VID_10C4&PID_EA61&MI_00.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_00
%USB\VID_10C4&PID_EA61&MI_01.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_01
%USB\VID_10C4&PID_EA61&MI_02.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_02
%USB\VID_10C4&PID_EA61&MI_03.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_03

[USBXpress_WinUSB.NTia64]
%USB\VID_10C4&PID_EA61.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61
%USB\VID_10C4&PID_EA61&MI_00.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_00
%USB\VID_10C4&PID_EA61&MI_01.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_01
%USB\VID_10C4&PID_EA61&MI_02.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_02
%USB\VID_10C4&PID_EA61&MI_03.DeviceDesc% =USB_Install, USB\VID_10C4&PID_EA61&MI_03

; =================== Installation ===================

[USB_Install]
Include=winusb.inf
Needs=WINUSB.NT

[USB_Install.Services]
Include=winusb.inf
AddService=WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\winusb.sys

[USB_Install.Wdf]
KmdfService=WINUSB, WinUsb_Install

[WinUSB_Install]
KmdfLibraryVersion=1.9

[USB_Install.HW]
AddReg=Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{3C5E1462-5695-4e18-876B-F3F3D08AAF18}"

[USB_Install.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

; ================= Source Media Section =====================

[SourceDisksNames]
1 = %DISK_NAME%,,,\x86
2 = %DISK_NAME%,,,\amd64
3 = %DISK_NAME%,,,\ia64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll=1
WdfCoInstaller01009.dll=1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll=2
WdfCoInstaller01009.dll=2

[SourceDisksFiles.ia64]
WinUSBCoInstaller2.dll=3
WdfCoInstaller01009.dll=3
; =================== Strings ===================

[Strings]
ProviderName="Silicon Laboratories"
USB\VID_10C4&PID_EA61.DeviceDesc="USBXpress Device"
USB\VID_10C4&PID_EA61&MI_00.DeviceDesc="USBXpress Device: Interface 0"
USB\VID_10C4&PID_EA61&MI_01.DeviceDesc="USBXpress Device: Interface 1"
USB\VID_10C4&PID_EA61&MI_02.DeviceDesc="USBXpress Device: Interface 2"
USB\VID_10C4&PID_EA61&MI_03.DeviceDesc="USBXpress Device: Interface 3"
WinUSB_SvcDesc="USBXpress WinUSB Service"
DISK_NAME="Silicon Labs USBXpress Driver Installation Disk"
